**Testing**  
  
**LED Lighting Up**

Check all leds light up when 5 V applied to inputs

**Input-Output Current Transfer**

check 24 V output switches on and off as expected with appropriate 5 V applied to each corresponding terminal

**No Shorts**

check there are no short circuits on the board